Table of Contents

#### Precautions ................................ 2

#### Revision History................................ 3

#### Foreword................................ 10

#### Brief Introduction 10

#### Chapter Outline 10

#### Chapter 1 Connecotni and Basic Settings 11

#### Introduction 11

#### Unpacking 11

#### Device Connection 11

#### USB Connection 12

#### RS232 Connection 13

#### Barcode Reading 14

#### Defaults Setting 15

#### Factory Default Setting 15

#### Chapter 2 Interface Type................................ 15

#### Introduction 15

#### RS232 16

#### RS232 Baud Rate 17

#### RS232 Word Length: Data Bits, Stop Bits, and Parity 18

#### USB 20

#### USB PC Keyboard 20

#### USB Serial 20

#### Chapter 3 Input/Output Settings 21

#### Introduction 21

#### Startup Beeper 21

#### Trigger Click Beeper 21

#### Good Read and Error Read Indicators 22

#### Good Read Beeper 22

#### Good Read Beeper Volume 22

#### Good Read Beeper Frequency 23

#### Good Read Beeper Duration 23

Error Read Beeper Frequency 23

Good Read LED 24

[Good Read Delay 25](#_TOC_250153)

[Chapter 4 Data Editing ................................ 26](#_TOC_250152)

[Introduction 26](#_TOC_250151)

Add Preﬁx or Suﬃx 27

[Example 28](#_TOC_250150)

[Add a Suﬃx to a speciﬁc symbology 28](#_TOC_250149)

[To Add a Carriage Return Suﬃx to All Symbologies 29](#_TOC_250148)

[To Add a Line Break Suﬃx to All Symbologies 29](#_TOC_250147)

[To Add a Carriage Return &a Line Break Suﬃx to All Symbologies 29](#_TOC_250146)

Keyboard Operation 30

Clear Preﬁxes or Suﬃxes 31

[Preﬁx Selections 31](#_TOC_250145)

[Suﬃx Selections 32](#_TOC_250144)

[Function Code Transmit 33](#_TOC_250143)

[Intermessage Delay 33](#_TOC_250142)

[Chapter 5 Symbologies ................................ 34](#_TOC_250141)

[Introduction 34](#_TOC_250140)

[All Symbologies 35](#_TOC_250139)

[Message Length Description 35](#_TOC_250138)

[1D Barcode 36](#_TOC_250137)

[2D Barcode 36](#_TOC_250136)

[Codabar 37](#_TOC_250135)

[On/Off 37](#_TOC_250134)

[Start/Stop Characters 37](#_TOC_250133)

[Check Character 37](#_TOC_250132)

[Concatenation 39](#_TOC_250131)

[Message Length 40](#_TOC_250130)

[Code 39 41](#_TOC_250129)

[Code 39 On/Off 41](#_TOC_250128)

[Start/ Stop Characters 41](#_TOC_250127)

[Check Character 42](#_TOC_250126)

[Message Length 42](#_TOC_250125)

[Code 39 Append 43](#_TOC_250124)

[Example 43](#_TOC_250123)

[Code 32 Pharmaceutical (PARAF) 44](#_TOC_250122)

[FULL ASCII 45](#_TOC_250121)

[Interleaved 2 of 5 46](#_TOC_250120)

[On/Off 46](#_TOC_250119)

[Check Digit 46](#_TOC_250118)

[Message Length 48](#_TOC_250117)

[NEC 2 of 5 49](#_TOC_250116)

[On/Off 49](#_TOC_250115)

[Check Digit 49](#_TOC_250114)

[Message Length 51](#_TOC_250113)

[Code 93 52](#_TOC_250112)

[On/Off 52](#_TOC_250111)

[Message Length 52](#_TOC_250110)

[Straight 2 of 5 Industrial (three-bar start/stop) 53](#_TOC_250109)

[On/Off 53](#_TOC_250108)

[Message Length 53](#_TOC_250107)

[Straight 2 of 5 IATA (two-bar start/stop) 54](#_TOC_250106)

[On/Off 54](#_TOC_250105)

[Message Length 54](#_TOC_250104)

[Matrix 2 of 5 55](#_TOC_250103)

[On/Off 55](#_TOC_250102)

[Message Length 55](#_TOC_250101)

[Check 56](#_TOC_250100)

[Code 11 57](#_TOC_250099)

[On/Off 57](#_TOC_250098)

[Check Digits Required 57](#_TOC_250097)

[Message Length 58](#_TOC_250096)

[Code 128 59](#_TOC_250095)

[On/Off 59](#_TOC_250094)

[ISBT 128 Concatenation 59](#_TOC_250093)

[Message Length 60](#_TOC_250092)

[GS1-128 61](#_TOC_250091)

[On/Off 61](#_TOC_250090)

[Message Length 61](#_TOC_250089)

[Telepen 62](#_TOC_250088)

[On/Off 62](#_TOC_250087)

[Message Length 62](#_TOC_250086)

[UPC-A 63](#_TOC_250085)

[Check Digit 63](#_TOC_250084)

[Number System 64](#_TOC_250083)

[Addenda 64](#_TOC_250082)

[Addenda Required 65](#_TOC_250081)

[Addenda Separator 65](#_TOC_250080)

[Note 65](#_TOC_250079)

[UPC-E0 66](#_TOC_250078)

[On/Off 66](#_TOC_250077)

[Expand 67](#_TOC_250076)

Addenda Required 67

[Addenda Separator 67](#_TOC_250075)

[Check Digit 68](#_TOC_250074)

[Number System 69](#_TOC_250073)

[Addenda 69](#_TOC_250072)

[UPC-E1 70](#_TOC_250071)

[EAN/JAN-13 70](#_TOC_250070)

[On/Off 70](#_TOC_250069)

[Check Digit 71](#_TOC_250068)

[Addenda 71](#_TOC_250067)

[Addenda Required 72](#_TOC_250066)

[Addenda Separator 72](#_TOC_250065)

[ISBN Translate 72](#_TOC_250064)

[EAN/JAN-8 73](#_TOC_250063)

[On/Off 73](#_TOC_250062)

[Check Digit 73](#_TOC_250061)

[Addenda 73](#_TOC_250060)

[Addenda Required 74](#_TOC_250059)

[Addenda Separator 74](#_TOC_250058)

[MSI 76](#_TOC_250057)

[On/Off 76](#_TOC_250056)

[Check Characte 77](#_TOC_250055)

[Message Length 77](#_TOC_250054)

[GS1 DataBar Omnidirectional 78](#_TOC_250053)

[On/Off 78](#_TOC_250052)

[GS1 DataBar Limited 78](#_TOC_250051)

[On/Off 78](#_TOC_250050)

[GS1 DataBar Expanded 79](#_TOC_250049)

[On/Off 79](#_TOC_250048)

[Message Length 79](#_TOC_250047)

[PDF417 80](#_TOC_250046)

[On/Off 80](#_TOC_250045)

[Message Length 80](#_TOC_250044)

[QR Code 81](#_TOC_250043)

[On/Off 81](#_TOC_250042)

[Message Length 81](#_TOC_250041)

[Data Matrix 82](#_TOC_250040)

On/Off 82

[Message Length 82](#_TOC_250039)

[Aztec Code 83](#_TOC_250038)

[On/Off 83](#_TOC_250037)

[Message Length 83](#_TOC_250036)

[China Post (Hong Kong 2 of 5) 84](#_TOC_250035)

[On/Off 84](#_TOC_250034)

[Message Length 84](#_TOC_250033)

[Korea Post 85](#_TOC_250032)

[On/Off 85](#_TOC_250031)

[Message Length 85](#_TOC_250030)

[Check Digit 86](#_TOC_250029)

[Han Xin Code 86](#_TOC_250028)

[On/Off 86](#_TOC_250027)

[Message Length 86](#_TOC_250026)

[Maxi code 88](#_TOC_250025)

[On/Off 88](#_TOC_250024)

[Message Length 88](#_TOC_250023)

[Micropdf 89](#_TOC_250022)

[On/Off 89](#_TOC_250021)

[Message Length 89](#_TOC_250020)

Composites 89

[On/Off 90](#_TOC_250019)

[Message Length 90](#_TOC_250018)

[Codablock A 91](#_TOC_250017)

[On/Off 91](#_TOC_250016)

[Message Length 91](#_TOC_250015)

[Codablock F 92](#_TOC_250014)

[On/Off 92](#_TOC_250013)

[Message Length 92](#_TOC_250012)

Chapter 6 Utilities 93

[Show Software Revision 93](#_TOC_250011)

[Chapter 7 Common Problems And Solutions 94](#_TOC_250010)

Chapter 8Maintenance And Customer Service 95

[Maintenance 95](#_TOC_250009)

[Customer Service 95](#_TOC_250008)

Reference Charts ................................ 96

[Symbology Charts 96](#_TOC_250007)

[Linear Symbologies 96](#_TOC_250006)

[2D Symbologies 98](#_TOC_250005)

[Postal Symbologies 99](#_TOC_250004)

[ASCII Conversion Chart 100](#_TOC_250003)

[Sample Symbols 103](#_TOC_250002)

[Programming Charts 107](#_TOC_250001)

[ASCII conversion of keyboard operation 110](#_TOC_250000)

# Foreword

## Brief Introduction

This manual provides bar code scanning equipment Start-up and conﬁguration instructions, as well as maintenance and customer support information.

## Chapter Outline

Chapter 1 Connections and Basic Settings :introduces the method and default settings for bar code scanning devices

Chapter 2 Interface Types : Describes the main conﬁguration of interface types Chapter 3 Input / Output Settings: Describes Conﬁguration Decoding

Success / Failed LED and Buzzer Response

Chapter 4 Data Editing Describes :How to Add Preﬁx / Suﬃx

Chapter 5 Code System :Introduces All Code Systems and Conﬁgurations Supported by Barcode Scanning Equipment

Chapter 6 Universal Features :provides software version display and factory default conﬁguration codes

Chapter 7 Common Problems and Solutions: List Common Problems and Solutions Chapter 8 Equipment Maintenance and Customer Service :Introduces Equipment

Maintenance and Customer Support Information

Appendix : provides commonly used code charts, etc.

# Chapter 1 Connection and Basic Settings

## Introduction

The barcode scanner supports three connection methods. Please follow the appropriate connection procedure to connect the barcode scanner.

## Unpacking

To open the product packaging, perform the following steps:

* Remove the scanner and its accessories and inspect for damage during shipment.
* Make sure the items in the carton match your order.
* If there are any damaged or missing parts, please contact your supplier for after-sales service

## Device Connection

The interface above the host is shown below:



USB USB interface on the host

RS232 RS232 interface on the host

**USB Connection**

The barcode scanner can be connected to the USB port of your computer.


1. Connect the device interface (RJ45 connector) of the USB cable to the device.
2. Connect the host interface (USB interface) of the USB cable to the host.
3. The barcode scanner is humming.
4. Verify the operation by scanning the Sample Symbols at the end of this manual.



##### RS232 Connection

1. Connect the device interface (RJ45 connector) of the RS-232 cable to the scanner.
2. Connect the host interface (RS-232 interface) of the RS-232 cable to the host.
3. The barcode scanner is humming.
4. Verify the operation by scanning the Sample Symbols at the end of this manual.

The interface is conﬁgured for 115,200 baud, 8 data bits, no parity and 1 stop bit.



The barcode scanner has a line of sight/point that projects a red aiming beam that corresponds to the horizontal ﬁeld of view of the barcode scanner. The line of sight/point should be at the center of the barcode, but it can be positioned in any direction to facilitate reading.


**Linearbarcode 2D Matrixsymbol**



The aiming beam or pattern is smaller when the barcode scanner is closer to the code and larger when it is farther from the code. Symbologies with smaller bars or elements (mil size) should be read closer to the unit. Symbologies with larger bars or elements (mil size) should be read farther from the unit. To read single or multiple symbols (on a page or on an object), hold the barcode scanner at an appropriate distance from the target, press the button, and center the aiming beam or pattern on the symbol. If the code being scanned is highly reﬂective (e.g., laminated), it may be necessary to tilt the code up 15°to 18°to prevent unwanted reﬂection.

## Factory Default Setting

Scan the "**Load Factory Defaults**" barcode below to reset the barcode scanner to the factory default settings.



(800006.)

**Load Factory Defaults**

# Chapter 2 Interface Type


## Introduction

This chapter introduces the USB and RS232 interface types and lists their

## RS232

related conﬁgurations.

Connect RS232 interface, you need to scan the "**RS232**" barcode, the serial port related conﬁguration is: 115200 baud rate, 8 data bits, no parity, 1 stop bit, add carriage return and line feed by default.



(8810010.)

**RS232**


## RS232 Baud Rate

Baud Rate sends the data from the scanner to the terminal at the speciﬁed rate. The host terminal must be set for the same baud rate as the scanner. Default =115200.




(8310030.)

**300**




(8310031.)

**600**




(8310032.)

**1200**




(8310033.)

**2400**




(8310034.)

**4800**




(8310035.)

**9600**




(8310036.)

**19200**




(8310037.)

**38400**



(8310038.)

**57,600**



(8310039.)


**\*115,200**

## RS232 Word Length: Data Bits, Stop Bits, and Parity

**Data Bits** You can choose to transfer 7,8-bit data bits, and you must set the terminal to the same data bit as the barcode scanner to communicate properly. Default = 8.


**Stop Bits** sets the stop bits at 1 or 2. Default = 1.

**Parity** provides a means of checking character bit patterns for validity. Default = None.




(8310063.)

**7 Data,1 Stop, Parity Even**




(8310060.)

**7 Data, 1 Stop , Parity None**




(8310066.)

**7 Data, 1 Stop, Parity Odd**




(8310064.)

**7 Data, 2 Stop, Parity Even**




(8310061.)

1. **Data, 2 Stop Parity None**




(8310065.)

1. **Data, 1 Stop, Parity Even**




(8310068.)

**8 Data, 1 Stop, Parity Odd**



(8310067.)

**7 Data, 2 Stop, Parity Odd**




(8310062.)

**\* 8 Data, 1 Stop, Parity None**

## USB


##### USB PC Keyboard

Scan one of the following code to program the scanner for USB PC Keyboard .Scanning these code also adds a CR and LF.

（881001124.）

**USB Keyboard (PC)**

##### USB Serial

Scan the following code to program the scanner to emulate a regular RS232- based COM Port.

(881001133.)

**USB Serial**


Note: No extra conﬁguration (e.g., baud rate) is necessary.

# Chapter 3 Input/Output Settings

## Introduction


This chapter mainly introduces the conﬁguration of the beep and LED of the barcode scanner when it is powered on, decoded, and triggered by the button.

## Startup Beeper

The scanner can be programmed to beep when it’s started up. Default = Startup Beeper On.

(8410130.)

**Startup Beeper Off**




（8410131.)

**\* Startup Beeper On**


## Trigger Click Beeper

To hear an audible click every time the scanner button is pressed, scan the **Trigger Click Beeper On** barcode below. Default = Trigger Click Beeper Off.



(8410140.)

**\*Trigger Click Beeper Off**




(8410141.)

**Trigger Click Beeper On**

## Good Read and Error Read Indicators

##### Good Read Beeper

The beeper may be programmed On or Off in response to a good read. Default = Good Read Beeper On.

(8410010.)

**Good Read Beeper Off**


##### Good Read Beeper Volume



(8410011.)

**\* Good Read Beeper On**

The beeper volume codes modify the volume of the beep the scanner emits on a good read. Default = High.




(8410091.)

**Low**




(8410092.)

**Medium**



(8410093.)

**\* High**




(8410090.)

**Off**


##### Good Read Beeper Frequency

The beeper frequency codes modify the frequency of the beep the scanner emits on a good read. Default = Medium.




(8410061600.)

**Low (1600 Hz)**



(8410062400.)

**\* Medium (2400 Hz)**




(8410064200.)

**High (4200 Hz)**

##### Good Read Beeper Duration


The beeper duration codes modify the length of the beep the scanner emits on a good read. Default = Normal .



(8410020.)

**\* Normal**


##### Error Read Beeper Frequency



(8410021.)

**Short**


The beeper frequency codes modify the frequency of the sound the scan- ner emits when there is a bad read or error. Default = Razz.




(841007250.)

**\* Razz (250 Hz)**

(8410073250.



**Medium (3250 Hz)**




(8410074200.)

**High (4200 Hz)**


##### Good Read LED

The LED indicator can be programmed **On** or **Off** in response to a good read. Default = On.



(8410081.)

**\* Good Read LED On**




(8410080.)

**Good Read LED Off**


##### Good Read Delay

This sets the minimum amount of time before the scanner can read another barcode. Default = \* Short Delay (750 ms)

.




(8510060.)

**No Delay**


(851006750.)

**\* Short Delay (750 ms)**



(8510061000.)

**Medium Delay (1,000 ms)**



(8510061500.)

**Long Delay (1,500 ms)**

# Chapter 4 Data Editing

## Introduction

This chapter describes how to add preﬁxes and suﬃxes.

* Default preﬁx = None. Default suﬃx = None.
* A preﬁx or suﬃx may be added or cleared from one symbology or all symbologies.
* You can add any preﬁx or suﬃx from the ASCII Conversion Chart deplus Code I.D. and AIM I.D.
* Enter preﬁxes and suﬃxes in the order in which you want them to appear on the output.
* When setting up for speciﬁc symbologies (as opposed to all symbologies), the speciﬁc symbology ID value counts as an added preﬁx or suﬃx character.
* The maximum size of a preﬁx or suﬃx conﬁguration is 200 characters, which includes header information.

## Add Preﬁx or Suﬃx

**Step 1.** Scan the **Add Preﬁx** or **Add Suﬃx** symbol

**Step 2.** Determine the 2 digit Hex value from the Symbology Chart for the symbology to which you want to apply the preﬁx or suﬃx. For example, for Code 11, Code ID is “h” and Hex ID is “68”.

**Step 3.** Scan the 2 hex digits from the Programming Chart inside the back cover of this manual or scan **9**, **9** for all symbologies.

**Step 4.** Determine the hex value from the ASCII Conversion Chart , for the preﬁx or suﬃx you wish to enter.

**Step 5.** Scan the 2 digit hex value from the Programming Chart inside the back cover of this manual.


**Step 6.** Repeat Steps 4 and 5 for every preﬁx or suﬃx character.

**Step 7.** To add the Code I.D., scan **5**, **C**, **8**, **0**.

To add AIM I.D., scan **5**, **C**, **8**, **1**.


To add a backslash (\), scan **5**, **C**, **5**, **C**.

**Step 8.** Scan **Save** to exit and save, or scan **Discard** to exit without saving.




(889002.)

**Add Preﬁx**




(888002.)

**Add Suﬃx**



(800002.)

**Save**

(800000.)

**Disgard**

## Example

##### Add a Suﬃx to a speciﬁc symbology

To send a CR (carriage return)Suﬃx for code 128. only:

**Step 1.** Scan **Add Suﬃx**.


**Step 2.** Determine the 2 digit hex value from the Symbology Charts for code 128.

**Step 3.** Scan **6**, **3** from the Programming Chart inside the back cover of this manual.


**Step 4.** Determine the hex value from the ASCII Conversion Chart , for the CR (carriage return).

**Step 5.** Scan **0**, **D** from the Programming Chart inside the back cover of this manual.

**Step 6.** Scan **Save**, or scan **Discard** to exit without saving.


(888002.)

**Add Suﬃx**




**(KAK.)**

**A**




**(SDS.)**

D



**(K6K.)**

6



**(K0K.)**


0

(800002.)

**Save**

##### To Add a Carriage Return Suﬃx to All Symbologies

Scan the following barcode if you wish to add a carriage return suﬃx to all symbologies at once. This action ﬁrst clears all current suﬃxes, then programs a carriage return suﬃx for all symbologies.




(890000.)

**Add CR Suﬃx All Symbologies**

##### To Add a Line Break Suﬃx to All Symbologies

Scan the following barcode if you wish to add a line break suﬃx to all symbologies at once. This action ﬁrst clears all current suﬃxes, then programs a line break suﬃx for all symbologies.




(888002990A.)

**Add LF Suﬃx All Symbologies**

##### To Add a Carriage Return &a Line Break Suﬃx to All Symbologies

Scan the following barcode if you wish to add a carriage return suﬃx and a line break suﬃx to all symbologies at once. This action ﬁrst clears all current suﬃxes, then programs a carriage return suﬃx and a line break suﬃx for all symbologies.



(888002990D0A.)

**Add CR and LF Suﬃx All Symbologies**

## Keyboard Operation

Different operations can be performed on the keyboard through conﬁguration during decoding output, such as automatic saving after decoding output.

Step 1: determine the hexadecimal value corresponding to the keyboard operation to be performed from the ASCII conversion of keyboard operation, and Determine the 2-digit hexadecimal value of the barcode to be set


Step 2. scan the barcode of "add keyboard operation".

Step 3. Determine the sequence of keyboard operation and barcode output. If keyboard operation is in front, scan "add preﬁx" barcode, and then scan "add suﬃx" barcode.

Step 4. Scan the corresponding 4-digit hexadecimal values in the Programming Charts of this manual according to the corresponding hexadecimal values (including barcode type and corresponding keyboard operation)


Step 5. Scan "save" barcode.

Step 6, scan "end adding keyboard operation"



（**8210042**）

**Add keyboard operation**



（**8210040**）

**End adding keyboard operation**

Example: add operation that automatic preservation after decoding output for all kinds of barcodes

First, conﬁrm the operation to be performed: save after barcode output, so suﬃx should be added after output barcode. Then determine the corresponding hexadecimal value according to the table in the appendix,all kinds of barcodes correspond to “9”“9”，The save operation corresponds to “1”“3”。

After conﬁrmation, scan "add keyboard operation" barcode, add suﬃx barcode, 9, 9, 1, 3, and then scan "save" barcode and “end adding keyboard operation” barcode

(Here "9" and "9" correspond to all coding systems, and "1" and "3" correspond to decoding output and saving)

## Clear Preﬁxes or Suﬃxes


You can clear a single preﬁx or suﬃx, or clear all preﬁxes/suﬃxes for a symbology. If you have been entering preﬁxes and suﬃxes for single sym- bologies, you can use **Clear One Preﬁx (Suﬃx)** to delete a speciﬁc char- acter from a symbology. When you **Clear All Preﬁxes (Suﬃxes)**, all the preﬁxes or suﬃxes for a symbology are deleted.

**Step 1.** Scan the **Clear One Preﬁx** or **Clear One Suﬃx** symbol.


**Step 2.** Determine the 2 digit Hex value from the Symbology Charts for the symbology from which you want to clear the preﬁx or suﬃx.

**Step 3.** Scan the 2 digit hex value from the Programming Chart inside the


back cover of this manual or scan **9**, **9** for all symbologies.

**Step 4.** Scan the **Save** symbol.

(889004.)

**Clear One Preﬁx**

**(888004.)**


**Clear One Suﬃx**

(800002.)

**Save**


## Preﬁx Selections

(889002.)

**Add Preﬁx**


(889004.)

**Clear One Preﬁx**

(889003.)


**Clear All Preﬁxes**

## Suﬃx Selections



(888002.)

**Add Suﬃx**



(888003.)

**Clear All Suﬃxes**




(888004.)

**Clear One Suﬃx**


## Function Code Transmit

When this selection is enabled and function codes are contained within the scanned data, the scanner transmits the function code to the terminal. Default = Disable.



(8080071.)

**\*Enable**



(8080070.)

**\*Disable**


## Intermessage Delay

An intermessage delay of up to 5000 milliseconds (in 5ms increments) may be placed between each scan transmission. Scan the **Intermessage Delay** barcode below, then scan the number of 5ms delays, and the **Save** barcode using the Programming Chart inside the back cover of this man- ual.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |

**1st Scan Transmission 2nd Scan Transmission**

**Intermessage Delay**



(851004.)

**Intermessage Delay**

To remove this delay, scan the **Intermessage Delay** barcode, then set the number of delays to 0. Scan the **Save** barcode using the Programming Chart inside the back cover of this manual.

Example: set a bar code **Intermessage Delay** of 100ms:

First scan " **Intermessage Delay** ", then scan "2" "0" from the Programming Chart (100 / 5 = 20), then scan "**save**" barcode.


# Chapter 5 Symbologies

## Introduction

Each type of barcode has its own unique properties. The barcode scanner can be adjusted to accommodate these property changes through the conﬁguration code in this chapter. The fewer the barcode types, the faster the barcode scanner can read. You can disable the barcode scanner to read the barcode types that will not be used to improve the performance of the barcode scanner.


## All Symbologies

If you want to decode all the symbologies allowable for your scanner, scan the **All Symbologies On** barcode. If on the other hand, you want to decode only a particular symbology, scan **All Symbologies Off** followed by the **On** barcode for that particular symbology.



(9990011.)

**All Symbologies On**



(9990010.)

**All Symbologies Off**

Note: When **All Symbologies On** is scanned, 2D Postal Codes are not enabled.

2D Postal Codes must be enabled separately.

## Message Length Description

You are able to set the valid reading length of some of the barcode symbolo- gies. If the data length of the scanned barcode doesn’t match the valid read- ing length, the scanner will issue an error tone. You may wish to set the same value for minimum and maximum length to force the scanner to read ﬁxed length barcode data. This helps reduce the chances of a misread.

**EXAMPLE:** Decode only those barcodes with a count of 6-10 characters.

Min. length = 06 Max. length = 10

**Step 1.** Select the barcode symbology to set the maximum reading length or the minimum reading length, scan the **Minimum Message Length** barcode in its catalog, and scan the number “**6**” and “**Save**” barcodes from the Programming Chart .

**Step 2.** Scan the **Maxmum Message Length** barcode and scan the numbers


**1**, **0** barcode and **Save** barcode from the Programming Chart . The above process sets the selected barcode symbology small reading length to 6 and the maximum reading length to 10

**EXAMPLE:** Decode only those barcodes with a count of 13 characters.

Min. length = 13 Max. length = 13


## 1D Barcode

If the bar code scanning device needs to decode all the one-dimensional code systems, please scan the bar code of “All 1D Barcode on”. Only solve speciﬁc code system, please scan " All 1D Barcode off" .



(9950040.)

**All 1D Barcode on**




## 2D Barcode

(9950041.)


**All 1D Barcode off**

If the bar code scanning device needs to decode all the two-dimensional code systems, please scan the bar code of “All 2D Barcode on”. Only solve speciﬁc code system, please scan " All 2D Barcode off"



(9950070.)


**All 2D Barcode on**



(9950071.)

**All 2D Barcode on**


## Codabar

**On/Off**

(9000031.)


**\* On**

## Start/Stop Characters




(900000.)

**Default All Codabar Settings**

(9000030.)


**Off**

Start/Stop characters identify the leading and trailing ends of the barcode. You may either transmit, or not transmit Start/Stop characters.Default = Don’t Transmit.



(9000061.)

**Transmit**



## Check Character


(9000060.)

**\* Don’t Transmit**


**No Check Character** indicates that the scanner reads and transmits barcode data with or without a check character.

When Check Character is set to **Validate and Transmit,** the scanner will only read Codabar barcodes printed with a check character, and will transmit this character at the end of the scanned data.

When Check Character is set to Validate, but Don’t Transmit, the unit will only read Codabar barcodes printed with a check character, but will not transmit the check character with the scanned data. Default = No Check Character.

(9000010.)


**\* No Check Character**



(9000012.)

**Validate and Transmit**

(9000011.)


**Validate but Don’t Transmit**


## Concatenation

Codabar supports symbol concatenation. When you enable concatena- tion, the scanner looks for a Codabar symbol having a “D” start character, adjacent to a symbol having a “D” stop character. In this case the two mes- sages are concatenated into one with the “D” characters omitted.

A 1 2 3 4 D D 5 6 7 8A

Select Require to prevent the scanner from decoding a single “D” Codabar symbol without its companion. This selection has no effect on Codabar symbols without Stop/Start D characters.




(9000021.)

**On**

(9000020.)


**\* Off**

(9000022.)

**Require**


## Message Length

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 2-60. Minimum Default = 4, Maximum Default = 60.



(900005.)

**Minimum Message Length**




(900004.)

**Maximum Message Length**

## Code 39

#### < Default All Code 39 Settings >




(901000.)

**Default All Code *39* Settings**

## Code 39 On/Off

(9010011.)

**\* On**




(9010010.)

**Off**


## Start/ Stop Characters

Start/Stop characters identify the leading and trailing ends of the barcode. You may either transmit, or not transmit Start/Stop characters. Default = Don’t Transmit.



(9010091.)

**Transmit**



(9010090.)


**\* Don’t Transmit**

## Check Character

**No Check Character** indicates that the scanner reads and transmits bar- code data with or without a check character.


When Check Character is set to **Validate, but Don’t Transmit**, the unit only reads Code 39 barcodes printed with a check character, but will not transmit the check character with the scanned data.

When Check Character is set to **Validate and Transmit**, the scanner only reads Code 39 barcodes printed with a check character, and will transmit this character at the end of the scanned data. Default = No Check Character.




(9010040.)

**\* No Check Character**



(9010041.)

**Validate, but Don’t Transmit**




(9010042.)

**Validate and Transmit**

## Message Length


Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths

= 0-48. Minimum Default = 0, Maximum Default = 48.



(901008.)

**Minimum Message Length**




(901007.)

**Maximum Message Length**

## Code 39 Append

This function allows the scanner to append the data from several Code 39 barcodes together before transmitting them to the host computer. When the scanner encounters a Code 39 barcode with the append trigger char- acter(s), it buffers Code 39 barcodes until it reads a Code 39 barcode that does not have the append trigger. The data is then transmitted in the order in which the barcodes were read (FIFO). Default = Off.




(9010021.)

**On**

## Example

(9010020.)

**\* Off**

After sanning **on** barcode, scan the three bar codes below in order. The barcode scanner does not output any data until the last bar code is scanned. After scanning the **ESS** barcode, the SUCCESS word is output correctly.

SU


**CC**

**ESS**

## Code 32 Pharmaceutical (PARAF)


Code 32 Pharmaceutical is a form of the Code 39 symbology used by Ital- ian pharmacies. This symbology is also known as PARAF.

When you conﬁgure code32, you need to turn on code39 before you conﬁgure it.



(9010051.)

**On**



(9010050.)


**\* Off**

## FULL ASCII

If Full ASCII Code 39 decoding is enabled, certain character pairs within the bar- code symbol will be interpreted as a single character. For example:$V will be decoded as the ASCII character SYN, and /C will be decoded as the ASCII character #. Default = Off.


|  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| NUL%U | DLE $P | SP SPACE | 0 | 0 | @%V | P | P | ‘ %W | p +P |
| SOH$A | DC1 $Q | ! /A | 1 | 1 | A A | Q | Q | a +A | q +Q |
| STX $B | DC2 $R | “ /B | 2 | 2 | B B | R | R | b +B | r +R |
| ETX $C | DC3 $S | # /C | 3 | 3 | C C | S | S | c +C | s +S |
| EOT $D | DC4 $T | $ /D | 4 | 4 | D D | T | T | d +D | t +T |
| ENQ $E | NAK $U | % /E | 5 | 5 | E E | U | U | e +E | u +U |
| ACK $F | SYN $V | & /F | 6 | 6 | F F | V | V | f +F | v +V |
| BEL $G | ETB $W | ‘ /G | 7 | 7 | G G | W | W | g +G | w +W |
| BS $H | CAN $X | ( /H | 8 | 8 | H H | X | X | h +H | x +X |
| HT $I | EM $Y | ) /I | 9 | 9 | I I | Y | Y | i +I | y +Y |
| LF $J | SUB $Z | \* /J | : | /Z | J J | Z | Z | j +J | z +Z |
| VT $K | ESC %A | + /K | ; | %F | K K | [ | %K | k +K | { %P |
| FF $L | FS %B | , /L | < | %G | L L | \ | %L | l +L | | %Q |
| CR $M | GS %C | - /M | = | %H | M M | ] | %M | m +M | } %R |
| SO $N | RS %D | . /N | > | %I | N N | ^ | %N | n +N | ~ %S |
| SI$O | US %E | / /O | ? | %J | O O | \_ | %O | o +O | DEL %T |

Character pairs /M and /N decode as a minus sign and period respectively. Character pairs /P through /Y decode as 0 through 9.



(9010031.)

**FULL ASCII On**




(9010030.)

**\* FULL ASCII Off**

## Interleaved 2 of 5


< Default All Interleaved 2 of 5 Settings >



## On/Off


(902000.)

**Default All Interleaved 2 of 5 Settings**



(9020021.)

**\* On**



## Check Digit


(9020020.)

**Off**

**No Check Digit** indicates that the scanner reads and transmits barcode data with or without a check digit.


When Check Digit is set to **Validate, but Don’t Transmit**, the unit only reads Interleaved 2 of 5 barcodes printed with a check digit, but will not transmit the check digit with the scanned data.


When Check Digit is set to **Validate and Transmit**, the scanner only reads Interleaved 2 of 5 barcodes printed with a check digit, and will transmit this digit at the end of the scanned data. Default = No Check Digit.



(9020010.)

**\* No Check Digit**





(9020012.)

**Validate and Transmit**


(9020011.)

**Validate, but Don’t Transmit**

## Message Length


Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths

= 2-80. Minimum Default = 4, Maximum Default = 80.



(902004.)


**Minimum Message Length**




(902003.)

**Maximum Message Length**

## NEC 2 of 5

**On/Off**

#### < Default All NEC 2 of 5 Settings >




(903000.)

**Default All NEC 2 of 5 Settings**

(9030011.)

**\* On**



(9030010.)


**Off**

## Check Digit

**No Check Digit** indicates that the scanner reads and transmits barcode data with or without a check digit.


When Check Digit is set to **Validate, but Don’t Transmit**, the unit only reads NEC 2 of 5 barcodes printed with a check digit, but will not transmit the check digit with the scanned data.


When Check Digit is set to **Validate and Transmit**, the scanner only reads NEC 2 of 5 barcodes printed with a check digit, and will transmit this digit at the end of the scanned data. Default = No Check Digit



(9030020.)

**\* No Check Digit**





(9030022.)

**Validate and Transmit**


(9030021.)

**Validate, but Don’t Transmit**

## Message Length


Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths

= 2-80. Minimum Default = 4, Maximum Default = 80.



(903004.)


**Minimum Message Length**




(903003.)

**Maximum Message Length**

## Code 93


**On/Off**

#### < Default All Code 93 Settings >



(904000.)

**Default All Code 93 Settings**

(9040021.)


**\* On**


(9040020.)

**Off**

## Message Length

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 0-80. Minimum Default = 0, Maximum Default = 80.



(904004.)


**Minimum Message Length**

(904003.)

**Maximum Message Length**

## Straight 2 of 5 Industrial (three-bar start/stop)

#### <Default All Straight 2 of 5 Industrial Settings>




(905000.)

**Default All Straight 2 of 5 Industrial (three-bar start/stop)Settings**

## On/Off

(9050011.)

**On**




(9050010.)

**\* Off**


## Message Length

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 1-48. Minimum Default = 4, Maximum Default = 48.



(905003.)

**Minimum Message Length**




(905002.)

**Maximum Message Length**


(906000.)

**Default All Straight 2 of 5 IATA (two-bar start/stop)Settings**

## On/Off

(9060011.)

**On**




## Message Length

（9060010.）


**Off**

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 1-48. Minimum Default = 4, Maximum Default = 48.




(906003.)

**Minimum Message Length**



(906002.)


**Maximum Message Length**



## On/Off


(907000.)

**Default All Matrix 2 of 5 Settings**



(9070011.)

**On**




## Message Length

(9070010.)


**\* Off**

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 1-80. Minimum Default = 4, Maximum Default = 80.



(907003.)

**Minimum Message Length**




(907002.)

**Maximum Message Length**


## Check

Scan the barcode below to enable or disable the check function of matrix25.



(9070051.)

**Enable Check Function**




(9070050.)

**Disable Check Function**

## Code 11


**On/Off**

#### <Default All Settings>




(908000.)

**Default All Code 11 Settings**



(9080021.)


**On**

(9080020.)

**\* Off**


## Check Digits Required

This option sets whether 1 or 2 check digits are required with Code 11 barcodes. Default = Two Check Digits.



(3110280.)

**One Check Digit**




(3110281.)

**\* Two Check Digits**


## Message Length

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 1-80. Minimum Default = 4, Maximum Default = 80.



(908004.)

**Minimum Message Length**




(908003.)

**Maximum Message Length**

## Code 128


#### <Default All Code 128 Settings>



(909000.)


**Default All Code 128 Settings**

## On/Off



(9090011.)


**\* On**



(9090010.)


**Off**

## ISBT 128 Concatenation



(9020051.)

**ISBT 128 On**




(9020050.)

**\*ISBT 128 Off**


## Message Length

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 0-80. Minimum Default = 0, Maximum Default = 80.



(909003.)

**Minimum Message Length**




(909002.)

**Maximum Message Length**

## GS1-128

<Default All GS1-128 Settings>



## On/Off


(9100011.)

**\* On**


## Message Length

(910000.)

**Default All GS1-128 Settings**


(9100010.)

**Off**

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 1-80. Minimum Default = 1, Maximum Default = 80.

(910003.)

**Minimum Message Length**




(910002.)

**Maximum Message Length**

## Telepen


<Default All Telepen Settings>



## On/Off


(911000.)

**Default All Telepen Settings**

(9110011.)


**On**

## Message Length




(9110010.)

**\* Off**

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 1-60. Minimum Default = 1, Maximum Default = 60.

(911003.)

**Minimum Message Length**




(911002.)

**Maximum Message Length**


## UPC-A

#### <Default All UPC-A Settings>




(912000.)

**Default All UPC-A Settings**

(9120031.)

**\* On**




(9120030.)

**Off**


## Check Digit

This selection allows you to specify whether the check digit should be transmitted at the end of the scanned data or not. Default = On.



(9120041.)

**\* On**




(9120040.)

**Off**


## Number System

The numeric system digit of a U.P.C. symbol is normally transmitted at the beginning of the scanned data, but the unit can be programmed so it will not transmit it. Default = On.



(9120051.)

**\* On**




## Addenda

(9120050.)


**Off**

This selection adds 2 or 5 digits to the end of all scanned UPC-A data. Default = Off for both 2 Digit and 5 Digit Addenda.




(9120011.)

**2 Digit Addenda On**




(9120010.)

**\* 2 Digit Addenda Off**



(9120021.)

**5 Digit Addenda On**




(9120020.)

**\* 5 Digit Addenda Off**


## Addenda Required

When **Required** is scanned, the scanner will only read UPC-A barcodes that have addenda. You must then turn on a 2 or 5 digit addenda. Default = Not Required.



(9120061.)

**Required**




## Addenda Separator

(9120060.)


**\* Not Required**

When this feature is on, there is a space between the data from the barcode and the data from the addenda. When turned off, there is no space. Default

= On*.*



(9120071.)


**\* On**

## Note

(9120070.)

**Off**

Scan the barcode below to convert UPC-A to EAN\_13 or not.



(9120111.)

**Convert**


(9120110.)

**Not convert**

## UPC-E0

**On/Off**


#### <Default All UPC-E Settings>



(914000.)


**Default All UPC-E0 Settings**

Most U.P.C. barcodes lead with the 0 number system. To read these codes, use the \***UPC-E0 On** selection. If you need to read codes that lead with the 1 number system, use UPC-E1. Default = On.



(9140101.)

**\* UPC-E0 On**




(9140100.)

**UPC-E0 Off**


## Expand

UPC-E Expand expands the UPC-E code to the 12 digit, UPC-A format. Default = Off.



(9140021.)

**On**




(9140020.)

**\* Off**


## Addenda Required

When **Required** is scanned, the scanner will only read UPC-E barcodes that have addenda. Default = Not Required.



(9140031.)

**Required**




## Addenda Separator

(9140030.)


**\* Not Required**

When this feature is On, there is a space between the data from the barcode and the data from the addenda. When turned Off, there is no space. Default = On



(9140041.)

**\* On**




## Check Digit

(9140040.)


**Off**

Check Digit speciﬁes whether the check digit should be transmitted at the end of the scanned data or not. Default = On.



(9140051.)

**\*On**




(9140050.)

**Off**


## Number System

The numeric system digit of a U.P.C. symbol is normally transmitted at the beginning of the scanned data, but the unit can be programmed so it will not transmit it. To prevent transmission, scan **Off**. Default = On*.*



(9140061.)

**\* On**




## Addenda

(9140060.)


**Off**

This selection adds 2 or 5 digits to the end of all scanned UPC-E data.Default = Off for both 2 Digit and 5 Digit Addenda.




(9140071.)

**2 Digit Addenda On**




(9140070.)

**\* 2 Digit Addenda Off**



(9140081.)

**5 Digit Addenda On**




(9140080.)

**\* 5 Digit Addenda Off**


## UPC-E1

Most U.P.C. barcodes lead with the 0 number system. For these codes, use UPC-E0. If you need to read codes that lead with the 1 number system, use the **UPC-E1 On** selection. Default = Off.



(9140091.)

**UPC-E1 On**




(9140090.)

**\* UPC-E1 Off**

**EAN/JAN-13**


<Default All EAN/JAN Settings>



(915000.)


**Default All EAN/JAN-13 Settings**

## On/Off



(9150011.)

**\*On**



(9150010.)


**Off**

Note: If you want to convert UPC-A barcodes to EAN-13 format, scan the

**UPC-A Off** barcode.


## Check Digit

This selection allows you to specify whether the check digit should be transmitted at the end of the scanned data or not. Default = On.



(9150021.)

**\* On**




(9150020.)

**Off**


## Addenda

This selection adds 2 or 5 digits to the end of all scanned EAN/JAN-13 data. Default = Off for both 2 Digit and 5 Digit Addenda.




(9150031.)

**2 Digit Addenda On**




(9150030.)

**\* 2 Digit Addenda Off**



(9150041.)

**5 Digit Addenda On**




(9150040.)

**\* 5 Digit Addenda Off**


## Addenda Required

When **Required** is scanned, the scanner will only read EAN/JAN-13 barcodes that have addenda. Default = Not Required.



(9150051.)

**Required**




## Addenda Separator

(9150050.)

**\* Not Required**


When this feature is **On**, there is a space between the data from the barcode and the data from the addenda. When turned **Off**, there is no space. Default

= On.



(9150061.)

**\* On**




## ISBN Translate

(9150060.)

**Off**

When **On** is scanned, EAN-13 Bookland symbols are translated into their equivalent ISBN number format. Default = Off.



(9150071.)

**On**

(9150070.)


**\* Off**


## EAN/JAN-8

<Default All EAN/JAN-8 Settings>

## On/Off


(916000.)

**Default All EAN/JAN-8 Settings**



**(9160011.)**

**\* On**




## Check Digit

(9160010.)


**Off**

This selection allows you to specify whether the check digit should be transmitted at the end of the scanned data or not. Default = On.



(9160021.)

**\* On**




## Addenda


(9160020.)

**Off**

This selection adds 2 or 5 digits to the end of all scanned EAN/JAN-8 data. Default = Off for both 2 Digit and 5 Digit *Addenda.*


(9160031.)

**2 Digit Addenda On**




(9160041.)

**5 Digit Addenda On**



(9160030.)

* **2 Digit Addenda Off**





(9160040.)

* **5 Digit Addenda Off**

## Addenda Required

When **Required** is scanned, the scanner will only read EAN/JAN-8 barcodes that have addenda. Default = Not Required.



(9160051.)

**Required**


(9160050.)

**\* Not Required**


## Addenda Separator

When this feature is **On**, there is a space between the data from the barcode and the data from the addenda. When turned **Off**, there is no space. Default

= On.



(9160061.)

**\* On**


(9160060.)

**Off**

## MSI


**On/Off**

#### *<*Default All MSI Settings*>*




(917000.)

**Default All MSI Settings**

(9170011.)

**On**



(9170010.)


**\* Off**

## Check Characte

MSI barcodes use different types of check characters. You can conﬁgure the barcode scanner to read the MSI barcode using the check character. Default = **Validate MOD 10, but Don’t Transmit**


When Check Character is set to **Validate MOD 10 and Transmit**, the scanner will only read MSI barcodes printed with the speciﬁed type check character(s), and will transmit the character(s) at the end of the scanned data.

When Check Character is set to **Validate MOD 10, but Don’t Transmit**, the unit will only read MSI barcodes printed with the speciﬁed type check character(s), but will not transmit the check character(s) with the scanned data.




(9170020.)

**\* Validate MOD 10, but Don’t Transmit**



(9170021.)

**Validate MOD 10 and Transmit**




(9170026.)

**Disable MSI Check Characters**


## Message Length

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 4-48. Minimum Default = 4, Maximum Default = 48.



(917004.)

**Minimum Message Length**




(917003.)

**Maximum Message Length**

## GS1 DataBar Omnidirectional

< Default All GS1 DataBar Omnidirectional Settings >




## On/Off

(918000.)

**Default All GS1 DataBar Omnidirectional Settings**

(9180011.)


**\* On**

## GS1 DataBar Limited

(9180010.)

**Off**


< Default All GS1 DataBar Limited Settings >




## On/Off

(919000.)

**Default All GS1 DataBar Limited Settings**

(9190011.)

**\* On**




(9190010.)

**Off**


## On/Off

(920000.)

**Default All GS1 DataBar Expanded Settings**

(9200011.)

**\* On**




(9200010.)

**Off**


## Message Length

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 4-74. Minimum Default = 4, Maximum Default = 74.



(920003.)

**Minimum Message Length**




(920002.)

**Maximum Message Length**

## On/Off

(924000.)


**Default All PD417 Settings**



(9240011.)

**\* On**


## Message Length



(9240010)


**Off**

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 1-2750. Minimum Default = 1, Maximum Default = 2750.



(924003.)

**Minimum Message Length**



(924002.)


**Maximum Message Length**

## On/Off

(928000.)


**Default All QR Code Settings**

This selection applies to both QR Code and Micro QR Code.



(9280011.)

**\* On**




## Message Length

(9280010.)


**Off**

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 1-7089. Minimum Default = 1, Maximum Default = 7089.




(928003.)

**Minimum Message Length**



(928002.)


**Maximum Message Length**




## On/Off

(930000.)

**Default All Data Matrix Settings**

(9300011.)


**\* On**



## Message Length (9300010.)


Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 1-3116. Minimum Default = 1, Maximum Default = 3116.

**Off**



(930002.)

**Minimum Message Length**




(930003.)

**Maximum Message Length**

## On/Off


(931000.)

**Default All Aztec Code Settings**



(9310011.)

**\* On**




## Message Length

(9310010.)


**off**

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 1-3832. Minimum Default = 1, Maximum Default = 3832.



(931003.)

**Minimum Message Length**




(931002.)

**Maximum Message Length**


(936000.)

**Default All China Post (Hong Kong 2 of 5)Settings**

## On/Off

(9360011.)

**On**




## Message Length

(9360010.)


**\* Off**

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 2-80. Minimum Default = 4, Maximum Default = 80.



(936003.)

**Minimum Message Length**




(936002.)

**Maximum Message Length**

## Korea Post


**On/Off**

#### <Default All Korea Post Settings>




(937000.)

**Default All Korea Post Settings**



(9370011.)

**On**




## Message Length

(9370010.)


**\* Off**

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 2-80. Minimum Default = 4, Maximum Default = 48.



(937003.)

**Minimum Message Length**




(937002.)

**Maximum Message Length**


## Check Digit

This selection allows you to specify whether the check digit should be transmitted at the end of the scanned data. Default = Don’t Transmit.



(9370041.)

**On**




## Han Xin Code

**On/Off**

(9370040.)


**\* Off**

<Default All Han Xin Code Settings>



(932000.)


**Default All Han Xin Code Settings**



(9320011.)

**On**


## Message Length



(9320010.)


**\* Off**

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 1-1000. Minimum Default = 1, Maximum Default = 1000.



(932003.)

**Minimum Message Length**




(932002.)


**Maximum Message Length**

## Maxi code

<defalt all maxi code settings>



## On/Off




(9290011.)

**On**


**(929000.)**

## Message Length

(9290010.)


**Off**

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 1-150. Minimum Default = 1, Maximum Default = 150.



(929003.)

**Minimum Message Length**



(929002.)


**Maximum Message Length**

## Micropdf

<defalt all micropdf settings>


## On/Off

(925000.)

**(9250011.)**

**On**


## Message Length



(9250010.)


**Off**

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 1-366. Minimum Default = 1, Maximum Default = 366.



(925003.)


**Minimum Message Length**



(925002.)


**Maximum Message Length**

## Composites

<defalt all composites settings>


## On/Off

(926000.)

**(9260011.)**

**On**


## Message Length



(9260010.)


**Off**

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 1-2435. Minimum Default = 1, Maximum Default = 2435.



(926004.)


**Minimum Message Length**



(926003.)


**Maximum Message Length**

## Codablock A

<defalt all composites settings>


## On/Off

(922000.)

**(9220011.)**

**On**


## Message Length



(9220010.)


**Off**

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 1-600. Minimum Default = 1, Maximum Default = 600.



(922003.)

**Minimum Message Length**




(922002.)

**Maximum Message Length**


## On/Off

(923000.)

**(9230011.)**

**On**


## Message Length



(9230010.)


**Off**

Scan the barcodes below to change the message length. Refer to Message Length Description for additional information. Minimum and Maximum lengths = 1-2048. Minimum Default = 1, Maximum Default = 2048.



(923003.)

**Minimum Message Length**



(923002.)

**Maximum Message Length**

**Disable GS1 Data Matrix**

## Scan the barcode to disable GS1 Data Matrix




On



Off

## Show Software Revision

Scan the barcode below to output the current software revision, unit serial number, and other product information.



(809004?.)

**Show Revision**

**Problem**: The barcode scanner does not work.

possible reason：

1. The barcode scanner is not powered, check the power of the equipment.
2. If you are using an incorrect cable, use the cable that was originally conﬁgured.
3. The cable interface is loose and reconnected.
4. Check if the button is normal.

**Problem**: The barcode scanner scans normally, but the data output is incorrect. possible reason：

1. The cable interface is loose and reconnected.
2. Barcode scanner may not be conﬁgured to display the correct terminal.
3. If you are using a USB to RS232 cable, if the data output is garbled, it may be that the data reception speed of the device does not match the output speed of the barcode scanner.

**Problem**: Barcode scanner does not decode some barcodes. possible reason：

1. The barcode is defective. Try to scan the same type of test barcode to see if it can be interpreted.
2. The distance between the barcode scanner and the barcode is not suitable. Please move closer or move away the barcode.
3. For barcodes with poor print quality, the preferred reading distance is 5-10 cm.
4. Conﬁrm that your device is enabled for this barcode type.

**Problem**: Other conditions cannot be decoded. possible reason：

1. Turn off the device power; properly connect the device to the barcode scanner; turn on the device and test it.
2. If the problem still cannot be solved, please contact the dealer or the manufacturer.

M aintenance

1. Stains and dust on the scanning window can sometimes affect the normal operation of the barcode scanner. When cleaning, use a good quality tissue to wipe gently, or use a soft cloth to clean.

If you use a paper with poor paper quality for a long time, it will damage the surface ﬁnish of the window and affect the reading effect of the barcode scanner.

1. The outer shell of the barcode scanner can be wiped with a soft, clean cloth. If necessary, add a small amount of detergent to the water, wipe it with a soft cloth and rub it.
2. Do not spray any liquid on the window.
3. The scanning window must be kept clean and the supplier is not liable for damage caused by improper maintenance.

### Customer Service

If you need help installing or troubleshooting a device, please contact us

**Reference Charts Symbology Charts Linear Symbologies**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Symbology** | AIM | | | |
| **ID** | **Possible Modiﬁers**  **（m）** | **ID** | Hex |
| **All Symbologies** |  |  |  | **99** |
| **Codabar** | ]Fm | 0-1 | a | **61** |
| **Code 11** | ]H3 |  | h | **68** |
| **Code 128** | ]Cm | 0, 1, 2, 4 | j | **6A** |
| **Code 32 Pharmaceutical (PARAF)** | ]X0 |  | < | **3C** |
| **Code 39 (supports Full ASCII mode)** | ]Am | 0, 1, 3, 4,  5,7 | b | **62** |
| **TCIF Linked Code 39 (TLC39)** | ]L2 |  | T | **54** |
| **Code 93 and 93i** | ]Gm | 0-9, A-Z, a-m | i | **69** |
| **EAN** | ]Em | 0, 1, 3, 4 | d | **64** |
| **EAN-13 (including Bookland EAN)** | ]E0 |  | d | **64** |
| **EAN-13 with Add-On** | ]E3 |  | d | **64** |
| **EAN-13 with Extended Coupon** | ]E3 |  | d | **64** |
| **EAN-8** | ]E4 |  | D | **44** |
| **EAN-8 with Add-On** | ]E3 |  | D | **44** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Symbology** | AIM | | | |
| **ID** | **Possible**  **Modiﬁers**  **（m）** | **ID** | **Hex** |
| **GS1** |  |  |  |  |
| **GS1 DataBar** | ]em | 0 | y | **79** |
| **GS1 DataBar Limited** | ]em |  | { | **7B** |
| **GS1 DataBar Expanded** | ]em |  | } | **7D** |
| **GS1-128** | ]C1 |  | I | **49** |
| **2 of 5** |  |  |  |  |
| **China Post (Hong Kong 2 of** | ]X0 |  | Q | **51** |
| **Interleaved 2 of 5** | ]Im | 0, 1, 3 | e | **65** |
| **Matrix 2 of 5** | ]X0 |  | m | **6D** |
| **NEC 2 of 5** | ]X0 |  | Y | **59** |
| **Straight 2 of 5 IATA** | ]Rm | 0, 1, 3 | f | **66** |
| **Straight 2 of 5 Industrial** | ]S0 |  | f | **66** |
| **MSI** | ]Mm | 0, 1 | g | **67** |
| **Telepen** | ]Bm |  | t | **74** |
| **UPC** |  | 0, 1, 2, 3,  8, |  |  |
| **UPC-A** | ]E0 |  | c | **63** |
| **UPC-A with Add-On** | ]E3 |  | c | **63** |
| **UPC-A with Extended Coupon** | ]E3 |  | c | **63** |
| **UPC-E** | ]E0 |  | E | **45** |
| **UPC-E with Add-On** | ]E3 |  | E | **45** |
| **UPC-E1** | ]X0 |  | E | **45** |
| **Add Code ID** |  |  |  | **5C**  **80** |
| **Add AIM Code ID** |  |  |  | **5C**  **81** |
| **Add Backslash** |  |  |  | **5C**  **5C** |
| **Batch Mode Quantilty** |  |  | 5 | **35** |

**5)**

9, A, B, C

## 2D Symbologies

6

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Symbology** | AIM | | | |
| **ID** | **Possible Modiﬁers**  **（m）** | **ID** | **Hex** |
| **All Symbologies** |  |  |  | **99** |
| **Aztec Code** | ]zm | 0-9, A-C | z | **7A** |
| **Chinese Sensible Code (Han Xin Code)** | ]X0 |  | H | **48** |
| **Codablock A** | ]O6 | 0, 1, 4, 5, | V | **56** |
| **Codablock F** | ]Om | 0, 1,64, 5, | q | **71** |
| **Code 49** | ]Tm | 0, 1, 2, 4 | l | **6C** |
| **Data Matrix** | ]dm | 0-6 | w | **77** |
| **GS1** | ]em | 0-3 | y | **79** |
| **GS1 Composite** | ]em | 0-3 | y | **79** |
| **GS1**  **DataBar Omnidirecti** | ]em | 0-3 | y | **79** |
| **MaxiCode** | ]Um | 0-3 | x | **78** |
| **PDF417** | ]Lm | 0-2 | r | **72** |
| **MicroPDF417** | ]Lm | 0-5 | R | **52** |
| **QR Code** | ]Qm | 0-6 | s | **73** |
| **Micro QR Code** | ]Qm |  | s | **73** |

**Postal Symbologies**

**Post**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Symbology** | AIM | | | |
| **ID** | **Possible Modiﬁers**  **（m）** | **ID** | **Hex** |
| **All Symbologies** |  |  |  | **99** |
| **Australian Post** | ]X0 |  | A | **41** |
| **British Post** | ]X0 |  | B | **42** |
| **Canadian Post** | ]X0 |  | C | **43** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Symbology** | AIM | | | |
| **ID** | **Possible Modiﬁer s** | **ID** | **Hex** |
| **China Post** | ]X0 | **（m）** | Q | **51** |
| **InfoMail** | ]X0 |  | , | **2c** |
| **Intelligent Mail Bar**  **Code** | ]X0 |  | M | **4D** |
| **Japanese Post** | ]X0 |  | J | **4A** |
| **KIX (Netherlands)** | ]X0 |  | K | **4B** |
| **Korea Post** | ]X0 |  | ? | **3F** |
| **Planet Code** | ]X0 |  | L | **4C** |
| **Postal-4i** | ]X0 |  | N | **4E** |
| **Postnet** | ]X0 |  | P | **50** |

## ASCII Conversion Chart

|  |  |  |
| --- | --- | --- |
| **Hex** | **Dec** | **Char** |
| 00 | 0 | NUL （Null char.） |
| 01 | 1 | SOH （Start of Header） |
| 02 | 2 | STX （Start of Text） |
| 03 | 3 | ETX （End of Text） |
| 04 | 4 | EOT （End of Transmission) |
| 05 | 5 | ENQ （Enquiry） |
| 06 | 6 | ACK （Acknowledgment） |
| 07 | 7 | BEL （Bell） |
| 08 | 8 | BS （Backspace） |
| 09 | 9 | HT （Horizontal Tab） |
| 0a | 10 | LF （Line Feed） |
| 0b | 11 | VT （Vertical Tab） |
| 0c | 12 | FF （Form Feed） |
| 0d | 13 | CR （Carriage Return） |
| 0e | 14 | SO （Shift Out） |
| 0f | 15 | SI （Shift In） |
| 10 | 16 | DLE （Data Link Escape） |
| 11 | 17 | DC1 （XON）（Device Control 1） |
| 12 | 18 | DC2 （Device Control 2） |
| 13 | 19 | DC3（XOFF）（Device Control 3） |
| 14 | 20 | DC4 （Device Control 4） |
| 15 | 21 | NAK （Negative Acknowledgment） |
| 16 | 22 | SYN （Synchronous Idle） |
| 17 | 23 | ETB （End of Trans. Block） |
| 18 | 24 | CAN （Cancel） |
| 19 | 25 | EM （End of Medium） |
| 1a | 26 | SUB （Substitute） |
| 1b | 27 | ESC （Escape） |
| 1c | 28 | FS （File Separator） |
| 1d | 29 | GS （Group Separator） |
| 1e | 30 | RS （Request to Send） |
| 1f | 31 | US （Unit Separator） |
| 20 | 32 | SP （Space） |
| 21 | 33 | ! （Exclamation Mark） |
| 22 | 34 | " （Double Quote） |
| 23 | 35 | # （Number Sign） |
| 24 | 36 | $ （Dollar Sign） |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | 25 | 37 | % （Percent） |  |
| 26 | 38 | & （Ampersand） |
| 27 | 39 | ` （Single Quote） |
| 28 | 40 | (（Right / Closing Parenthesis） |
| 29 | 41 | )（Right / Closing Parenthesis） |
| 2a | 42 | \* （Asterisk） |
| 2b | 43 | + （Plus） |
| 2c | 44 | ,（Comma） |
| 2d | 45 | -（Minus / Dash） |
| 2e | 46 | . （Dot） |
| 2f | 47 | / （Forward Slash） |
| 30 | 48 | 0 |
| 31 | 49 | 1 |
| 32 | 50 | 2 |
| 33 | 51 | 3 |
| 34 | 52 | 4 |
| 35 | 53 | 5 |
| 36 | 54 | 6 |
| 37 | 55 | 7 |
| 38 | 56 | 8 |
| 39 | 57 | 9 |
| 3a | 58 | ：（Colon） |
| 3b | 59 | ；（Semi-colon） |
| 3c | 60 | < （Less Than） |
| 3d | 61 | = （Equal Sign） |
| 3e | 62 | > （Greater Than） |
| 3f | 63 | ? （Question Mark） |
| 40 | 64 | @ （AT Symbol） |
| 41 | 65 | A |
| 42 | 66 | B |
| 43 | 67 | C |
| 44 | 68 | D |
| 45 | 69 | E |
| 46 | 70 | F |
| 47 | 71 | G |
| 48 | 72 | H |
| 49 | 73 | I |
| 4a | 74 | J |
| 4b | 75 | K |
| 4c | 76 | L |
| 4d | 77 | M |
| 4e | 78 | N |
| 4f | 79 | O |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | 50 | 80 | P |  |
| 51 | 81 | Q |
| 52 | 82 | R |
| 53 | 83 | S |
| 54 | 84 | T |
| 55 | 85 | U |
| 56 | 86 | V |
| 57 | 87 | W |
| 58 | 88 | X |
| 59 | 89 | Y |
| 5a | 90 | Z |
| 5b | 91 | [ （Left / Opening Bracket） |
| 5c | 92 | \（Back Slash） |
| 5d | 93 | ] （Right / Closing Bracket） |
| 5e | 94 | ^ （Caret / Circumﬂex） |
| 5f | 95 | \_ （Underscore） |
| 60 | 96 | ' （Grave Accent） |
| 61 | 97 | a |
| 62 | 98 | b |
| 63 | 99 | c |
| 64 | 100 | d |
| 65 | 101 | e |
| 66 | 102 | f |
| 67 | 103 | g |
| 68 | 104 | h |
| 69 | 105 | i |
| 6a | 106 | j |
| 6b | 107 | k |
| 6c | 108 | l |
| 6d | 109 | m |
| 6e | 110 | n |
| 6f | 111 | o |
| 70 | 112 | p |
| 71 | 113 | q |
| 72 | 114 | r |
| 73 | 115 | s |
| 74 | 116 | t |
| 75 | 117 | u |
| 76 | 118 | v |
| 77 | 119 | w |
| 78 | 120 | x |
| 79 | 121 | y |
| 7a | 122 | z |
| 7b | 123 | { （Left/ Opening Brace） |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | 7c | 124 | | （Vertical Bar） |  |
| 7d | 125 | } （Right/Closing Brace） |
| 7e | 126 | ~ （Tilde） |
| 7f | 127 | DEL （Delete） |


**Sample Symbols**

###### UPC-A

01234567890 **Interleaved 2 of 5**



Code 128



###### Straight 2 of 5Industrial

123456

###### Matrix 2 of 5

6543210


###### Code 93

123456-9$ **Straight 2 of 5Industrial**

###### Matrix 2 of 5

123456

6543210 **GS1DataBar**



###### PDF417

Codabar

Data Matrix

###### QRCode




Numbers

TestSymbol

###### Aztec




**MaxiCode**




Test Message

###### Micro PDF417




Test Message

## Programming Charts




(K0K.)

**0**




(K2K.)

**2**




(K4K.)

**4**




(K6K.)

**6**




(K1K.)

**1**




(K3K.)

**3**



(K5K.)


**5**




(K7K.)

**7**

(K8K.)




**8**




(KAK.)

**A**




(KCK.)

**C**




(KEK.)

**E**




(K9K.)




**(KBK.)**

**B**




(KDK.)

**D**




(KFK.)

**F**



(800002.)

**Save**



(800000.)

**Discard**

Note: If an error occurs while scanning a letter or number (before scanning the "**Save**" barcode), scan the "**Discard**" barcode, rescan the correct letter or number, and then scan the "**Save**" barcode.

## ASCII conversion of keyboard operation

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **HEX** | **DEC** | **CTRL+X** | **FUNCTION** | |
| **00** | **0** | **CTRL+@** |  |  |
| **01** | **1** | **CTRL+A** | **Select all** |  |
| **02** | **2** | **CTRL+B** | **Bold** |  |
| **03** | **3** | **CTRL+C** | **Copy** |  |
| **04** | **4** | **CTRL+D** | **Bookmark** |  |
| **05** | **5** | **CTRL+E** | **Center** |  |
| **06** | **6** | **CTRL+F** | **Find** |  |
| **07** | **7** | **CTRL+G** |  |  |
| **08** | **8** | **CTRL+H** | **History** |  |
| **09** | **9** | **CTRL+I** |  |  |
| **0a** | **10** | **CTRL+J** | **Justify** |  |
| **0b** | **11** | **CTRL+K** | **Hyperlink** |  |
| **0c** | **12** | **CTRL+L** |  |  |
| **0d** | **13** | **CTRL+M** |  |  |
| **0e** | **14** | **CTRL+N** | **New** |  |
| **0f** | **15** | **CTRL+O** | **Open** |  |
| **10** | **16** | **CTRL+P** | **Print** |  |
| **11** | **17** | **CTRL+Q** | **Quit** |  |
| **12** | **18** | **CTRL+R** |  |  |
| **13** | **19** | **CTRL+S** | **save** |  |
| **14** | **20** | **CTRL+T** |  |  |
| **15** | **21** | **CTRL+U** |  | F12 |
| **16** | **22** | **CTRL+V** | **Paste** | F1 |
| **17** | **23** | **CTRL+W** |  | F2 |
| **18** | **24** | **CTRL+X** |  | F3 |
| **19** | **25** | **CTRL+Y** |  | F4 |
| **1a** | **26** | **CTRL+Z** |  | F5 |
| **1b** | **27** | **CTRL+[** |  | F6 |
| **1c** | **28** | **CTRL+\** |  | F7 |
| **1d** | **29** | **CTRL+]** |  | F8 |
| **1e** | **30** | **CTRL+^** |  | F9 |
| **1f** | **31** | **CTRL+-** |  | F10 |
| **7f** | 32 | CTRL+ |  |  |